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2026 Emulsified Asphalt Proficiency Samples 85 (A) and 86 (B)
 Data Sheet

 Closing Date: October 15, 2026

We encourage you to use the online data entry system to submit your results If your laboratory is not registered to submit results online, or if there are questions, contact AASHTO re:source at psp@aashtoresource.org or call 240-436-4900.

Testing Emulsified Asphalts - Enter Test Results in Rows (1) to (11) Below
	
	Sample 85 (A)
	Sample 86 (B)

	Saybolt Furol Viscosity at 25°C (77°F):
      Mark the Box to Show the Method Used – T59 |_|, D7496 |_|
	
	

	Saybolt Furol Viscosity (nearest 0.1 s) 	(1)
	
	

	Rotational Paddle Viscosity at 25°C (77°F) 
Mark the Box to Show the Method Used – T 382|_|, D7226 |_| Device Used: DPV |_|, TE-DPV |_|
	
	

	Apparent Viscosity at 25°C (nearest 0.1 mPa-s) 	 (2)
	
	

	Tests on the Residue by Distillation:
Mark the Box to Show the Method Used – T59 |_|, D6997 |_|
	
	

	Percent Residue (nearest 0.1 percent) 	(3)
	
	

	Percent Oil Distillate by Volume of Emulsion (nearest 0.1 percent) 	(4)
	
	

	Penetration of Distillation Residue
Mark the Box to Show the Method Used – T49 |_|, D5 |_|
	
	

	Penetration of the Residue at 25°C (nearest whole unit) 	..(5)
	
	

	Solubility of the Distillation Residue
Mark the Box to Show the Method Used – T44 |_|, D2042 |_|
	
	

	Percent Solubility of the Residue (nearest 0.01 percent) 	(6)
	
	

	Tests on the Residue by Evaporation:
Mark the Box to Show the Method Used – T59 |_|, D6934 |_|
	
	

	Percent Residue- average of beakers (nearest 0.1 percent) 	(7)
	
	

	Mark the Box to Show the Method Used – T49 |_|, D5 |_|
	
	

	Penetration of the Residue at 25°C (nearest whole unit) 	(8)
	
	

	Mark the Box to Show the Method Used – T44 |_|, D2042 |_|
Solvent Used:  Trichlorethylene |_|, Trichloroethane |_|, Toluene |_|, n-Propyl Bromide |_|
	
	

	Percent Solubility of the Residue (nearest 0.01 percent) 	(9)
	
	

	Ash Content:
Mark the Box to Show the Method Used – T111 |_|, D8078 |_|
Method used to collect residue: 
Evaporation: T59 |_|, D6934 |_| or Distillation: T59 |_|, D6997 |_|
	
	

	Ash Content of the Residue (nearest 0.01 percent) 	(10)
	
	

	Optional Study: 
Percent Residue by Quick Boil (ASTM D8476)
Mass of specimen used: Sample 85 (A):_____ 86 (B):_____

	
	

	Percent Residue (nearest 0.1 percent) 	(11)
	
	



Please report the following information to identify your laboratory:
	Name:
	

	Lab Number:
	

	City, State, Country:
	

	Submitted by:
	

	Phone:
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